I-6605

**OC Section:** [[F-7600]](#7600) New OC Section: 09 Navigation and Entertainment / Acoustic Vehicle Alerting System (AVAS)

**Description:**

UC "Pedestrian Warning System Usage"

Preconditions

- driving below approximately 32 km/h or while driving in reverse

Main Scenario

- Car emit sound out\_27, because EV operate quietly, and this sound helps to alert pedestrians of your oncoming vehicle

Post conditions

- Pedestrians know that car is near

**Priority:** Normal

**Type**: Use Case CF